## Atheros Client Utility Help

Introduction System Requirements Profile Management Create or Modify a Profile Remove a Profile Profile Auto Selection Switch Profiles Configure TCP/IP Configuring Win XP Security EAP-FAST EAP-TLS EAP-TTLS PEAP (EAP-GTC) PEAP (EAP-MSCHAP V2) LEAP WPA Passphrase Check Status or Diagnostics Check Current Status Check Driver Information Check Statistics Connect to Another Network Settings Signal Strength Display Data Display Display Refresh Interval Tools Tray Icon Troubleshooting Utility Enable/ Disable the Radio |  | ### Using LEAP Security To use security In the Atheros Client Utility, access the Security tab in the Profile Management window. LEAP security requires that all infrastructure devices (e.g. access points and servers) are configured for LEAP authentication. Check with the IT manager.
| Configuring LEAP
| Enabling LEAP
Enabling LEAP
| On the Security tab, choose the WPA radio button. Choose WPA-LEAP from the drop-down menu.
| OR: On the Security tab, choose the 802.1x radio button. Choose LEAP from the drop-down menu.
Click the Configure button. Specify a user name and password: Select to Use Temporary User Name and Password by choosing the radio button:
| Check Use Windows User Name to use the Windows user name as the LEAP user name.
| OR: Check Manually Prompt for LEAP User Name and Password to manually enter a user name and password and start the LEAP authentication process. The system then prompts the user for a user name and password on each login, or when the user chooses Manual LEAP Login from the Action menu.
Select to Use Saved User Name and Password by choosing the radio button:
| Specify the LEAP user name, password, and domain to to automatically authenticate on each login.
Enter the user name and password. Confirm the password. Specify a domain name:
| Check the Include Windows Logon Domain with User Name setting to pass the Windows login domain and user name to the RADIUS server. (default)
| OR: Enter a specific domain name.
If desired, check No Network Connection Unless User Is Logged In to force the wireless adapter to disassociate after logging off. Enter the LEAP authentication timeout time (between 30 and 500 seconds) to specify how long LEAP should wait before declaring authentication failed, and sending an error message. The default is 90 seconds. Click OK. Enable the profile.