## Atheros Client Utility Help

Introduction System Requirements Profile Management Create or Modify a Profile Remove a Profile Profile Auto Selection Switch Profiles Configure TCP/IP Configuring Win XP Security EAP-FAST EAP-TLS EAP-TTLS PEAP (EAP-GTC) PEAP (EAP-MSCHAP V2) LEAP WPA Passphrase Check Status or Diagnostics Check Current Status Check Driver Information Check Statistics Connect to Another Network Settings Signal Strength Display Data Display Display Refresh Interval Tools Tray Icon Troubleshooting Utility Enable/ Disable the Radio |  | ### Profile Management Configure the wireless network adapter (wireless card) from the Profile Management tab of the Atheros Client Utility.
| Add a profile
| Edit a profile
| Import a Profile
| Export a Profile
| Order profiles
| Switch to a different profile
| Remove a profile
| Connect to a Different Network
The wireless network adapter works in either infrastructure mode (which uses an access point) or ad hoc mode (a group of stations participating in the wireless LAN). Highlight a configuration profile in the profile list to find out details for that profile including network type, security mode, and the SSIDs (network names) associated with that profile.