Nejdelší nám známý spoj s použitím COMPEX WPE54AG-2A13EU

Dostala se nám do rukou velmi zajímavá reference od zákazníka , který má nasazen spoj na 17km se zařízeními COMPEX WPE54AG v režimu Wireless Bridge Link.

Rádi se o jeho zkušenosti podělíme :

Na 17km nám běží momentálně spoj se dvěmi NetPassage WPE54AG  v režimu Wireless Bridge Link s dvěmi sítovými parabolami 29dBi

System Up Time	2 months 7 days 13:39:27	
Firmware Version	2.07 Build 0067, Jan 3 2006	
 
Jede to spolehlivě za každého počasí. 
Když hustě prší sníží se propustnost na 2Mbity, ale pak se to zas samo rozjede a stabilně to běží na 6Mbitech FullDuplex (plný vysílací výkon s použítím úzce směrových antén).Abych řekl pravdu, vůbec o tom zařízení nevím. (*POZOR dle těchto údajů zákazník překračuje vysílací limit ČTU )
Popravdě tento starší model se na tuto velkou vzdálenost chová tedy lépe než ten novější WP54AG co jsme tam měli původně. Ten jel také ale jen na 2Mbitech FullDuplex.
Ten nový WP54AG máme ted na spoji 5km, z města na vesnici. V té oblasti je docela rušení. 
Z počátku jsme s ním měli problémy, ale vyřešilo to když jsme ručně otestovali pár kanálů a vybrali nejstabilnější. Po 14dnech jsme ho vyladili, rychlost nastavili manuálně na 6Mb FullDuplex a ted jede také naprosto v pohodě. 

Tak jako tak můžu oba vřele doporučit. 
Co se týče nastavování a ovládání, je to lepší než u konkurenčních zařízení. Ovládání je jednoduché, přehledné. 
Celkem je škoda, že to neumí zobrazit v Site Survey všechny sítě ve všech režimech které podporuje. 
Na anténách na 2.4Ghz jsem schopen chytat i 5Ghz a naopak. Je to tak, mám to ozkoušené. Hodí se to když v té lokalitě začnou problémy tak se můžu podívat kdo tam zas co spustil. Ale to není až tak velká chyba.
Naopak to má rychlé odezvy, hlavně při zaměřování. Site survey se zobrazí celkem okamžitě. Na detailní doladení pak používáme statistiku, je přesnější. 

Z našeho pohledu se oba tyto modely hodí do více náročných prostředí. Pokud se spoj dobře nainstaluje, tak o něm nevíte. 

Parametry našeho spoje jsou :  (Sítová parabola 29dBi , vzdálenost 17km )
 
krátký ping :  --- ping statistics ---
326 packets transmitted, 326 received, 0% packet loss, time 325292ms
rtt min/avg/max/mdev = 2.319/4.025/34.986/4.302 ms, pipe 2
 
Delší flood  : --- ping statistics ---
5174 packets transmitted, 5160 received, 0% packet loss, time 403514ms
rtt min/avg/max/mdev = 2.326/998.589/1363.710/483.418 ms, pipe 18, ipg/ewma 78.003/905.173 ms
(spoj si packety cachuje, bohužel jsem to stopnul ve chvíli kdy je nestihl ještě zapsat.)

Link Statistics	
State	Power Save		
associated	off		

Encryption	Advertised Cipher	Unicast Cipher	Multicast Cipher	
no	None	None	None	

Authentication	Deauthentication	Association	Disassociation	Reassociation	
0	0	0	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	26337979	 	26371886	 	0	 	0	 	0	 	0	
Transmit	 	24998608	 	24998608	 	0	 	0	 	0	 	0	

 	 	Signal Strength (RSSI)	 	Data Rate (Mbps)	
Receive	 	16	 	48	
Transmit	 	21	 	48   |  48	

Receive
Errors	Discarded
Frames	Duplicate
Frames	CRC
Errors	Decrypt
Errors	PHY
Errors	DMA
Errors	
0	33907	33907	0	0	0	0	

Transmit
Errors	Discarded
Frames	Excessive
Retries	DMA
Errors	
0	0	0	0	

AP Statistics	
Authentication Type	Encryption	Cipher Advertised	
Open-System	no	None	

Authentication	Deauthentication	Association	Disassociation	Reassociation	
0	0	0	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	26300053	 	26333882	 	0	 	0	 	0	 	8128180	
Transmit	 	25060389	 	25060389	 	92564	 	0	 	0	 	0	

Receive
Errors	Discarded
Frames	Duplicate
Frames	CRC
Errors	Decrypt
Errors	PHY
Errors	DMA
Errors	
8128180	33854	33829	7660743	0	467437	0	

Transmit
Errors	Discarded
Frames	Excessive
Retries	DMA
Errors	
0	0	0	0	
 
protistrana
 
AP Statistics	
Authentication Type	Encryption	Cipher Advertised	
Open-System	no	None	

Authentication	Deauthentication	Association	Disassociation	Reassociation	
0	0	0	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	82764889	 	84034201	 	0	 	0	 	0	 	28820731	
Transmit	 	92703055	 	92703348	 	348181	 	0	 	0	 	6231	

Receive
Errors	Discarded
Frames	Duplicate
Frames	CRC
Errors	Decrypt
Errors	PHY
Errors	DMA
Errors	
28820731	1269312	1269312	28087396	0	733335	0	

Transmit
Errors	Discarded
Frames	Excessive
Retries	DMA
Errors	
6231	293	0	0	

Link Statistics	
State	Power Save		
associated	off		

Encryption	Advertised Cipher	Unicast Cipher	Multicast Cipher	
no	None	None	None	

Authentication	Deauthentication	Association	Disassociation	Reassociation	
0	0	0	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	82801382	 	84070963	 	0	 	0	 	0	 	0	
Transmit	 	92400131	 	92400424	 	0	 	0	 	0	 	6231	

 	 	Signal Strength (RSSI)	 	Data Rate (Mbps)	
Receive	 	19	 	48	
Transmit	 	23	 	54   |  54	

Receive
Errors	Discarded
Frames	Duplicate
Frames	CRC
Errors	Decrypt
Errors	PHY
Errors	DMA
Errors	
0	1269581	1269581	0	0	0	0	

Transmit
Errors	Discarded
Frames	Excessive
Retries	DMA
Errors	
6231	293	0	0	

 

POZOR  - Dle udávaného RSSI a výpočtu  pro tuto vzdálenost zákazník překračuje povolený maximální vysílací výkon pro toto pásmo (ERIP), na což jsme ho upozornili ! Pokud se vysílací výkon nastaví dle limitu tak spoj funguje, ale jen na rychlosti cca 2Mbit hd.

 
Druhý spoj na 5km WP54AG 

Device:	
System Up Time :	30 Days 03:37:00 	
BIOS/Loader Version :	2.1f (build 0310) 	
Firmware Version :	1.43 (build 0628) 	
NetWork Mode :	Inherent Bridge	
TxRate	54Mbps	
Signal Strength	28	
 
Authentication Type	Encryption	
Open	No	

Authentication	Deauthentication	Association	Disassociation	Reassociation	
1	0	1	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	5836103	 	5836103	 	0	 	25427579	 	0	 	952	
Transmit	 	9506011	 	9506011	 	0	 	60	 	0	 	0	
 
protistrana
 
Statistics
Authentication	Deauthentication	Association	Disassociation	Reassociation	
1	0	1	0	0	

 	 	MSDU	 	Data	 	Multicast	 	Management	 	Control	 	Errors	
Receive	 	3386390	 	3386390	 	0	 	2	 	0	 	0	
Transmit	 	2109558	 	2109558	 	0	 	3	 	0	 	0	

Spoj jede stabilně 6Mbit FullDuplex (omezeno), nemám v tudle chvíli možnost otestovat větší rychlosti.