## Atheros Client Utility Help

Introduction System Requirements Profile Management Create or Modify a Profile Remove a Profile Profile Auto Selection Switch Profiles Configure TCP/IP Configuring Win XP Security EAP-FAST EAP-TLS EAP-TTLS PEAP (EAP-GTC) PEAP (EAP-MSCHAP V2) LEAP WPA Passphrase Check Status or Diagnostics Check Current Status Check Driver Information Check Statistics Connect to Another Network Settings Signal Strength Display Data Display Display Refresh Interval Tools Tray Icon Troubleshooting Utility Enable/ Disable the Radio |  | ### Uninstall an Old Driver Uninstall an old driver before upgrading to a new NDIS driver release. To remove the newly installed driver from the system if the system does not have previously installed versions of the NDIS driver, proceed to Step 4. To remove the NDIS driver from the OS, go to Device Manager, right-click Atheros AR500x Wireless Network Adapter, and choose Uninstall. Click OK to uninstall the device. When the device is uninstalled from Device Manager, search for and delete the driver files that reside in the system. Go to the Start menu and choose Search > For Files or Folders. Enter oem*.inf in the Search for files or folders named: field, and enter Atheros in the Containing text: field. Click Search Now. A few files matching these criteria are possible, if previous drivers have not been removed properly. Choose the files that have been found and delete them from the system. To complete the uninstallation, remove the file ar5211.sys from the folder \WINNT\system32\drivers.